# tn_connect.update

Update TrueNAS Connect configuration.

Type: object

##

Type: array
No Additional Items

#### Tuple Validation

##### Parameter 1: tn_connect_update

#### tn_connect_update

Type: object

TrueNASConnectUpdateArgs parameters.

No Additional Properties

##

#### Enabled

Type: boolean

##

#### Ips

Type: array of string
No Additional Items

##### Each item of this array must be:

Type: string Format: ipvanyaddress

##

#### Account Service Base Url

Type: string Format: uri

Must be at least `1` characters long

Must be at most `2083` characters long

##

#### Leca Service Base Url

Type: string Format: uri

Must be at least `1` characters long

Must be at most `2083` characters long

##

#### Tnc Base Url

Type: string Format: uri

Must be at least `1` characters long

Must be at most `2083` characters long

##

#### Heartbeat Url

Type: string Format: uri

Must be at least `1` characters long

Must be at most `2083` characters long

##

#### TrueNASConnectEntry

Type: object
No Additional Properties

##

#### Id

Type: integer

##

#### Enabled

Type: boolean

##

#### Registration Details

Type: object

##

#### Ips

Type: array of string
No Additional Items

##### Each item of this array must be:

Type: string

Must be at least `1` characters long

##

#### Status

Type: string

Must be at least `1` characters long

##

#### Status Reason

Type: string

Must be at least `1` characters long

##

#### Certificate

## Any of

Type: integer
Type: null

##

#### Account Service Base Url

Type: string Format: uri

Must be at least `1` characters long

Must be at most `2083` characters long

##

#### Leca Service Base Url

Type: string Format: uri

Must be at least `1` characters long

Must be at most `2083` characters long

##

#### Tnc Base Url

Type: string Format: uri

Must be at least `1` characters long

Must be at most `2083` characters long

##

#### Heartbeat Url

Type: string Format: uri

Must be at least `1` characters long

Must be at most `2083` characters long

Required roles: TRUENAS_CONNECT_WRITE