# iscsi.portal.listen_ip_choices

Returns possible choices for listen.ip attribute of portal create and update.

Type: object

##

Type: array
No Additional Items

##

#### Result

Type: object

Object mapping IP addresses to their underlying constituents. Only static IP addresses will be included. On ALUA-enabled high availability systems, VIPs will be mapped to the pair of corresponding underlying addresses, one per node.

##

Each additional property must conform to the following schema

Type: string

Required roles: READONLY_ADMIN | SHARING_ISCSI_PORTAL_READ