# interface.xmit_hash_policy_choices

Available transmit hash policies for the LACP or LOADBALANCE lagg type interfaces.

Type: object

##

Type: array
No Additional Items

##

#### InterfaceXmitHashPolicyChoicesResult

Type: object

InterfaceXmitHashPolicyChoicesResult return fields.

No Additional Properties

##

#### Layer2

Type: const

Use MAC addresses for traffic distribution across bond members.

Specific value: `"LAYER2"`

##

#### Layer2+3

Type: const

Use MAC and IP addresses for traffic distribution across bond members.

Specific value: `"LAYER2+3"`

##

#### Layer3+4

Type: const

Use MAC, IP, and TCP/UDP port information for traffic distribution across bond members.

Specific value: `"LAYER3+4"`

Required roles: NETWORK_INTERFACE_READ | READONLY_ADMIN