# ipmi.chassis.identify

Toggle the chassis identify light.

verb: str if ‘ON’ turn identify light on. if ‘OFF’ turn identify light off. apply_remote: bool if True on HA systems, apply to remote controller.

Type: object

##

Type: array
No Additional Items

#### Tuple Validation

##### Parameter 1: verb

#### verb

Type: enum (of string) Default: "ON"

Action to perform on the chassis identify LED.

##### Must be one of:

- "ON"
- "OFF"

##

#### Result

Type: null

Returns `null` when the chassis identify operation completes successfully.

Required roles: IPMI_WRITE