# virt.global.get_network

Details for the given network.

Type: object

##

Type: array
No Additional Items

#### Tuple Validation

##### Parameter 1: name

#### name

Type: string

Name of the network configuration to retrieve.

Must be at least `1` characters long

##

#### VirtGlobalGetNetworkResult

Type: object

VirtGlobalGetNetworkResult return fields.

No Additional Properties

##

#### Type

Type: const

Type of network configuration (currently only bridge networks are supported).

Specific value: `"BRIDGE"`

##

#### Managed

Type: boolean

Whether this network is managed by the virtualization system.

##

#### Ipv4 Address

Type: string

IPv4 address and CIDR of the bridge network.

Must be at least `1` characters long

##

#### Ipv4 Nat

Type: boolean

Whether IPv4 Network Address Translation is enabled for this bridge.

##

#### Ipv6 Address

Type: string

IPv6 address and CIDR of the bridge network.

Must be at least `1` characters long

##

#### Ipv6 Nat

Type: boolean

Whether IPv6 Network Address Translation is enabled for this bridge.

Required roles: VIRT_GLOBAL_READ