# ipmi.chassis.identify

Toggle the chassis identify light.

verb: str if ‘ON’ turn identify light on. if ‘OFF’ turn identify light off. apply_remote: bool if True on HA systems, apply to remote controller.

Type: object

##

Type: array
No Additional Items

#### Tuple Validation

##### Parameter 1: data

#### data

Type: object

Request parameters for IPMI chassis identify operation.

No Additional Properties

##

#### Verb

Type: enum (of string) Default: "ON"

Action to perform on the chassis identify LED.

##### Must be one of:

- "ON"
- "OFF"

##

#### Apply Remote

Type: boolean Default: false

If on an HA system, and this field is set to True, the settings will be sent to the remote controller.

##

#### Result

Type: null

Returns `null` when the chassis identify operation completes successfully.

Required roles: IPMI_WRITE