# nvmet.subsys.update

Update NVMe target subsystem (subsys) of id.

Type: object

##

Type: array
No Additional Items

#### Tuple Validation

##### Parameter 1: id

#### id

Type: integer

ID of the subsystem to update.

##### Parameter 2: nvmet_subsys_update

#### nvmet_subsys_update

Type: object

Updated configuration data for the NVMe-oF subsystem.

No Additional Properties

##

#### Name

Type: string

Human readable name for the subsystem.

If `subnqn` is not provided on creation, then this name will be appended to the `basenqn` from `nvmet.global.config` to generate a subnqn.

Must be at least `1` characters long

##

#### Subnqn

NVMe Qualified Name (NQN) for the subsystem.

Must be a valid NQN format if provided.

## Any of

Type: string

Must be at least `11` characters long

Must be at most `223` characters long

Type: null

##

#### Allow Any Host

Type: boolean

Any host can access the storage associated with this subsystem (i.e. no access control).

##

#### Pi Enable

Enable Protection Information (PI) for data integrity checking.

## Any of

Type: boolean
Type: null

##

#### Qid Max

Maximum number of queue IDs allowed for this subsystem.

## Any of

Type: integer
Type: null

##

#### Ieee Oui

IEEE Organizationally Unique Identifier for the subsystem.

## Any of

Type: string
Type: null

##

#### Ana

If set to either `True` or `False`, then override the global `ana` setting from `nvmet.global.config` for this subsystem only.

If `null`, then the global `ana` setting will take effect.

## Any of

Type: boolean
Type: null

##

#### NVMetSubsysEntry

Type: object

The updated NVMe-oF subsystem configuration.

No Additional Properties

##

#### Id

Type: integer

Unique identifier for the NVMe-oF subsystem.

##

#### Name

Type: string

Human readable name for the subsystem.

If `subnqn` is not provided on creation, then this name will be appended to the `basenqn` from `nvmet.global.config` to generate a subnqn.

Must be at least `1` characters long

##

#### Subnqn

Default: null

NVMe Qualified Name (NQN) for the subsystem.

If not provided during creation, will be auto-generated by appending the `name` to the `basenqn` from `nvmet.global.config`.

## Any of

Type: string

Must be at least `1` characters long

Type: null

##

#### Serial

Type: string

Serial number assigned to the subsystem.

##

#### Allow Any Host

Type: boolean Default: false

Any host can access the storage associated with this subsystem (i.e. no access control).

##

#### Pi Enable

Default: null

Enable Protection Information (PI) for data integrity checking.

## Any of

Type: boolean
Type: null

##

#### Qid Max

Default: null

Maximum number of queue IDs allowed for this subsystem.

## Any of

Type: integer
Type: null

##

#### Ieee Oui

Default: null

IEEE Organizationally Unique Identifier for the subsystem.

## Any of

Type: string
Type: null

##

#### Ana

Default: null

If set to either `True` or `False`, then override the global `ana` setting from `nvmet.global.config` for this subsystem only.

If `null`, then the global `ana` setting will take effect.

## Any of

Type: boolean
Type: null

##

#### Hosts

Default: []

List of host ids which have access to this subsystem.

Only populated on query if `extra.options.verbose` is set.

## Any of

Type: array of integer
No Additional Items

##### Each item of this array must be:

Type: integer
Type: null

##

#### Namespaces

Default: []

List of namespaces ids in this subsystem.

Only populated on query if `extra.options.verbose` is set.

## Any of

Type: array of integer
No Additional Items

##### Each item of this array must be:

Type: integer
Type: null

##

#### Ports

Default: []

List of ports ids on which this subsystem is available.

Only populated on query if `extra.options.verbose` is set.

## Any of

Type: array of integer
No Additional Items

##### Each item of this array must be:

Type: integer
Type: null

Required roles: SHARING_NVME_TARGET_WRITE