# tn_connect.config

Sent on TrueNAS Connect configuration changes

Type: object

##

#### TrueNASConnectConfigChangedEvent

Type: object
No Additional Properties

##

#### TrueNASConnectEntry

Type: object

Event data.

No Additional Properties

##

#### Id

Type: integer

Unique identifier for the TrueNAS Connect configuration.

##

#### Enabled

Type: boolean

Whether TrueNAS Connect service is enabled.

##

#### Registration Details

Type: object

Object containing registration information and credentials for TrueNAS Connect.

##

#### Ips

Type: array of string

Array of IP addresses that TrueNAS Connect will bind to and advertise.

No Additional Items

##### Each item of this array must be:

Type: string

Must be at least `1` characters long

##

#### Interfaces

Type: array of string

Array of network interface names that TrueNAS Connect will use.

No Additional Items

##### Each item of this array must be:

Type: string

##

#### Interfaces Ips

Type: array of string

Array of IP addresses associated with the selected interfaces.

No Additional Items

##### Each item of this array must be:

Type: string

##

#### Use All Interfaces

Type: boolean

Whether to automatically use all available network interfaces.

##

#### Status

Type: string

Current operational status of the TrueNAS Connect service.

Must be at least `1` characters long

##

#### Status Reason

Type: string

Detailed explanation of the current status, including any error conditions.

Must be at least `1` characters long

##

#### Certificate

ID of the SSL certificate used for TrueNAS Connect communications. `null` if using default.

## Any of

Type: integer
Type: null

##

#### Account Service Base Url

Type: string Format: uri

Base URL for the TrueNAS Connect account service API.

Must be at least `1` characters long

Must be at most `2083` characters long

##

#### Leca Service Base Url

Type: string Format: uri

Base URL for the Let's Encrypt Certificate Authority service used by TrueNAS Connect.

Must be at least `1` characters long

Must be at most `2083` characters long

##

#### Tnc Base Url

Type: string Format: uri

Base URL for the TrueNAS Connect service.

Must be at least `1` characters long

Must be at most `2083` characters long

##

#### Heartbeat Url

Type: string Format: uri

URL endpoint for sending heartbeat signals to maintain connection status.

Must be at least `1` characters long

Must be at most `2083` characters long

Required roles: TRUENAS_CONNECT_READ