# ups.update

Update UPS Service Configuration.

powerdown when enabled, sets UPS to power off after shutting down the system.

nocommwarntime is a value in seconds which makes UPS Service wait the specified seconds before alerting that the Service cannot reach configured UPS.

shutdowntimer is a value in seconds which tells the Service to wait specified seconds for the UPS before initiating a shutdown. This only applies when shutdown is set to “BATT”.

shutdowncmd is the command which is executed to initiate a shutdown. It defaults to “poweroff”.

Type: object

##

Type: array
No Additional Items

#### Tuple Validation

##### Parameter 1: ups_update

#### ups_update

Type: object

UPSUpdateArgs parameters.

No Additional Properties

##

#### Powerdown

Type: boolean

Whether the UPS should power down after completing the shutdown sequence.

##

#### Rmonitor

Type: boolean

Whether to enable remote monitoring of the UPS status over the network.

##

#### Nocommwarntime

Seconds to wait before warning about communication loss with UPS. `null` for default.

## Any of

Type: integer
Type: null

##

#### Remoteport

Type: integer

Network port for communicating with remote UPS monitoring systems.

Value must be greater or equal to `1` and lesser or equal to `65535`

##

#### Shutdowntimer

Type: integer

Seconds to wait after initiating shutdown before forcing power off.

##

#### Hostsync

Type: integer

Maximum seconds to wait for other systems to shutdown before continuing.

Value must be greater or equal to `0`

##

#### Description

Type: string

Human-readable description of this UPS configuration.

##

#### Driver

Type: string

UPS driver name that handles communication with the specific UPS hardware model.

##

#### Extrausers

Type: string

Additional user configurations for UPS monitoring access.

##

#### Identifier

Type: string

Unique identifier name for this UPS device within the monitoring system.

Must be at least `1` characters long

##

#### Mode

Type: enum (of string)

Operating mode.
* `MASTER` controls the UPS directly
* `SLAVE` monitors remotely

##### Must be one of:

- "MASTER"
- "SLAVE"

##

#### Monpwd

Type: string

Password for UPS monitoring authentication (required for updates).

Must be at least `1` characters long

##

#### Monuser

Type: string

Username for UPS monitoring authentication.

Must be at least `1` characters long

##

#### Options

Type: string

Additional configuration options passed to the UPS driver.

##

#### Optionsupsd

Type: string

Additional configuration options for the UPS daemon.

##

#### Port

Type: string

Serial port or device path for UPS communication.

##

#### Remotehost

Type: string

Hostname or IP address of remote UPS server when operating in SLAVE mode.

##

#### Shutdown

Type: enum (of string)

Shutdown trigger condition: LOWBATT on low battery, BATT when on battery power.

##### Must be one of:

- "LOWBATT"
- "BATT"

##

#### Shutdowncmd

Custom command to execute during UPS shutdown sequence. `null` for default.

## Any of

Type: string
Type: null

##

#### UPSEntry

Type: object

The updated UPS configuration.

No Additional Properties

##

#### Powerdown

Type: boolean

Whether the UPS should power down after completing the shutdown sequence.

##

#### Rmonitor

Type: boolean

Whether to enable remote monitoring of the UPS status over the network.

##

#### Id

Type: integer

Unique identifier for the UPS configuration.

##

#### Nocommwarntime

Seconds to wait before warning about communication loss with UPS. `null` for default.

## Any of

Type: integer
Type: null

##

#### Remoteport

Type: integer

Network port for communicating with remote UPS monitoring systems.

Value must be greater or equal to `1` and lesser or equal to `65535`

##

#### Shutdowntimer

Type: integer

Seconds to wait after initiating shutdown before forcing power off.

##

#### Hostsync

Type: integer

Maximum seconds to wait for other systems to shutdown before continuing.

Value must be greater or equal to `0`

##

#### Description

Type: string

Human-readable description of this UPS configuration.

##

#### Driver

Type: string

UPS driver name that handles communication with the specific UPS hardware model.

##

#### Extrausers

Type: string

Additional user configurations for UPS monitoring access.

##

#### Identifier

Type: string

Unique identifier name for this UPS device within the monitoring system.

Must be at least `1` characters long

##

#### Mode

Type: enum (of string)

Operating mode.
* `MASTER` controls the UPS directly
* `SLAVE` monitors remotely

##### Must be one of:

- "MASTER"
- "SLAVE"

##

#### Monpwd

Type: string

Password for UPS monitoring authentication.

##

#### Monuser

Type: string

Username for UPS monitoring authentication.

Must be at least `1` characters long

##

#### Options

Type: string

Additional configuration options passed to the UPS driver.

##

#### Optionsupsd

Type: string

Additional configuration options for the UPS daemon.

##

#### Port

Type: string

Serial port or device path for UPS communication.

##

#### Remotehost

Type: string

Hostname or IP address of remote UPS server when operating in SLAVE mode.

##

#### Shutdown

Type: enum (of string)

Shutdown trigger condition: LOWBATT on low battery, BATT when on battery power.

##### Must be one of:

- "LOWBATT"
- "BATT"

##

#### Shutdowncmd

Custom command to execute during UPS shutdown sequence. `null` for default.

## Any of

Type: string
Type: null

##

#### Complete Identifier

Type: string

Complete UPS identifier including hostname for network monitoring.

Required roles: SYSTEM_GENERAL_WRITE