# failover.update

Update failover configuration.

Type: object

##

Type: array
No Additional Items

#### Tuple Validation

##### Parameter 1: data

#### data

Type: object

Updated failover configuration data.

No Additional Properties

##

#### Disabled

Type: boolean

When true, HA will be administratively disabled.

##

#### Master

Type: boolean

Marks the particular node in the chassis as the master node. The standby node will have the opposite value.

##

#### Timeout

Type: integer

The time to WAIT (in seconds) until a failover occurs when a network event occurs on an interface that is marked critical for failover AND HA is enabled and working appropriately. The default time to wait is 2 seconds.

NOTE: This setting does NOT effect the `disabled` or `master` parameters.

##

#### FailoverEntry

Type: object

The updated failover configuration.

No Additional Properties

##

#### Id

Type: integer

Unique identifier for the failover configuration.

##

#### Disabled

Type: boolean

When true, HA will be administratively disabled.

##

#### Master

Type: boolean

Marks the particular node in the chassis as the master node. The standby node will have the opposite value.

##

#### Timeout

Type: integer

The time to WAIT (in seconds) until a failover occurs when a network event occurs on an interface that is marked critical for failover AND HA is enabled and working appropriately. The default time to wait is 2 seconds.

NOTE: This setting does NOT effect the `disabled` or `master` parameters.

Required roles: FAILOVER_WRITE