# failover.reboot.info

Return reboot information for both nodes of the failover pair.

The response reports, for the local node and for the other node, whether a reboot is required and the reasons for it. The `other_node` field is `null` when the remote node cannot be reached.

Type: object

##

Type: array
No Additional Items

##

#### FailoverRebootInfoResult

Type: object

FailoverRebootInfoResult return fields.

No Additional Properties

##

#### RebootInfo

Type: object

Reboot information for the current node.

No Additional Properties

##

#### Boot Id

Type: string

Unique identifier for the current boot session.

##

#### Reboot Required Reasons

Type: array of object

Array of reasons why a system reboot is required.

No Additional Items

##### Each item of this array must be:

#### RebootRequiredReason

Type: object
No Additional Properties

##

#### Code

Type: string

Code identifying the reason for required reboot.

##

#### Reason

Type: string

Human-readable description of why a reboot is required.

##

Reboot information for the other node in the failover pair or `null` if not available.

## Any of

#### RebootInfo

Type: object
No Additional Properties

##

#### Boot Id

Type: string

Unique identifier for the current boot session.

##

#### Reboot Required Reasons

Type: array

Array of reasons why a system reboot is required.

No Additional Items

##### Each item of this array must be:

Type: object
Type: null

Required roles: FAILOVER_READ