# ipmi.chassis.info

Return IPMI chassis info.

On an HA system, set `query-remote` to `true` to return the chassis info from the remote controller instead of the local one.

Type: object

##

Type: array
No Additional Items

#### Tuple Validation

##### Parameter 1: data

#### data

Type: object

Request parameters for IPMI chassis information.

No Additional Properties

##

#### Query-Remote

Type: boolean Default: false

Whether to query remote IPMI chassis information on HA systems.

##

#### Result

IPMI chassis information or raw dictionary if parsing fails.

## Any of

#### IPMIChassisInfo

Type: object
No Additional Properties

##

#### System Power

Type: string

Current system power state.

Examples:

    "on"

    "off"

##

#### Power Overload

Type: string

Power overload status indicator.

##

#### Interlock

Type: string

Chassis interlock status.

##

#### Power Fault

Type: string

Power fault status indicator.

##

#### Power Control Fault

Type: string

Power control fault status indicator.

##

#### Power Restore Policy

Type: string

Policy for restoring power after a power loss.

##

#### Last Power Event

Type: string

Description of the last power-related event.

##

#### Chassis Intrusion

Type: string

Chassis intrusion detection status.

##

#### Front Panel Lockout

Type: string

Front panel lockout status indicator.

##

#### Drive Fault

Type: string

Drive fault status indicator.

##

#### Cooling/Fan Fault

Type: string

Cooling fan fault status indicator.

##

#### Chassis Identify State

Type: string

Current chassis identify LED state.

Type: object

Required roles: IPMI_READ