# vm.device.get_instance

Returns instance matching id. If id is not found, Validation error is raised.

Please see query method documentation for options.

Type: object

##

Type: array
No Additional Items

#### Tuple Validation

##### Parameter 1: id

#### id

Type: integer

##### Parameter 2: options

#### options

Type: object Default: {}

Query options customize the results returned by a query method. More complete documentation with examples are covered in the "Query methods" section of the TrueNAS API documentation.

No Additional Properties

##

#### Extra

Type: object Default: {}

Extra options are defined on a per-endpoint basis and are described in the documentation for the associated query method.

##

#### Order By

Type: array of string Default: []

An array of field names describing the manner in which query results should be ordered. The field names may also have one of more of the following special prefixes: `-` (reverse sort direction), `nulls_first:` (place any null values at the head of the results list), `nulls_last:` (place any null values at the tail of the results list).

No Additional Items

##### Each item of this array must be:

Type: string
Example:

    [
        "size",
        "-devname",
        "nulls_first:-expiretime"
    ]

##

#### Select

Type: array Default: []

An array of field names specifying the exact fields to include in the query return. The dot character `.` may be used to explicitly select only subkeys of the query result.

No Additional Items

##### Each item of this array must be:

## Any of

Type: string
Type: array
No Additional Items

##### Each item of this array must be:

Type: object
Example:

    [
        "username",
        "Authentication.status"
    ]

##

#### Count

Type: boolean Default: false

Return a numeric value representing the number of items that match the specified `query-filters`.

##

#### Get

Type: boolean Default: false

Return the JSON object of the first result matching the specified `query-filters`. The query fails if there specified `query-filters` return no results.

##

#### Offset

Type: integer Default: 0

This specifies the beginning offset of the results array. When combined with the `limit` query-option it may be used to implement pagination of large results arrays. WARNING: some query methods provide volatile results and the onus is on the developer to understand whether pagination is appropriate for a particular query API method.

##

#### Limit

Type: integer Default: 0

This specifies the maximum number of results matching the specified `query-filters` to return. When combined wtih the `offset` query-option it may be used to implement pagination of large results arrays.

WARNING: Some query methods provide volatile results and the onus is on the developer to understand whether pagination is appropriate for a particular query API method.

##

#### Force Sql Filters

Type: boolean Default: false

Force use of SQL for result filtering to reduce response time. May not work for all methods.

##

#### VMDeviceEntry

Type: object
No Additional Properties

##

#### Id

Type: integer

Unique identifier for the VM device.

##

#### Attributes

Device-specific configuration attributes.

## One of

#### VMCDROMDevice

Type: object
No Additional Properties

##

#### Dtype

Type: const

Device type identifier for CD-ROM/DVD devices.

Specific value: `"CDROM"`

##

#### Path

Type: string Default: "*"

Path must not contain "{", "}" characters, and it should start with "/mnt/".

Must match regular expression: `^[^{}]*$`

Must be at least `1` characters long

#### VMDisplayDevice

Type: object
No Additional Properties

##

#### Dtype

Type: const

Device type identifier for display/graphics devices.

Specific value: `"DISPLAY"`

##

#### Resolution

Type: enum (of string) Default: "1024x768"

Screen resolution for the virtual display.

##### Must be one of:

- "1920x1200"
- "1920x1080"
- "1600x1200"
- "1600x900"
- "1400x1050"
- "1280x1024"
- "1280x720"
- "1024x768"
- "800x600"
- "640x480"

##

#### Port

Default: null

VNC/SPICE port number for remote display access. `null` for auto-assignment.

## Any of

Type: integer

Value must be greater or equal to `5900` and lesser or equal to `65535`

Type: null

##

#### Web Port

Default: null

Web-based display access port number. `null` for auto-assignment.

## Any of

Type: integer
Type: null

##

#### Bind

Type: string Default: "127.0.0.1"

IP address to bind the display server to.

Must be at least `1` characters long

##

#### Wait

Type: boolean Default: false

Whether to wait for a client connection before starting the VM.

##

#### Password

Default: null

Password for display server authentication.

## Any of

Type: string
Type: null

##

#### Web

Type: boolean Default: true

Whether to enable web-based display access.

##

#### Type

Type: enum (of string) Default: "SPICE"

Display protocol type.

##### Must be one of:

- "SPICE"
- "VNC"

#### VMNICDevice

Type: object
No Additional Properties

##

#### Dtype

Type: const

Device type identifier for network interface cards.

Specific value: `"NIC"`

##

#### Trust Guest Rx Filters

Type: boolean Default: false

Whether to trust guest OS receive filter settings for better performance.

##

#### Type

Type: enum (of string) Default: "E1000"

Network interface controller type. `E1000` for Intel compatibility, `VIRTIO` for performance.

##### Must be one of:

- "E1000"
- "VIRTIO"

##

#### Nic Attach

Default: null

Host network interface or bridge to attach to. `null` for no attachment.

## Any of

Type: string
Type: null

##

#### Mac

Default: null

MAC address for the virtual network interface. `null` for auto-generation.

## Any of

Type: string
Must match regular expression: `^([0-9A-Fa-f]{2}[:-]?){5}([0-9A-Fa-f]{2})$`
Type: null

#### VMPCIDevice

Type: object
No Additional Properties

##

#### Dtype

Type: const

Device type identifier for PCI passthrough devices.

Specific value: `"PCI"`

##

#### Pptdev

Type: string

Host PCI device identifier to pass through to the VM.

Must be at least `1` characters long

#### VMRAWDevice

Type: object
No Additional Properties

##

#### Dtype

Type: const

Device type identifier for raw disk devices.

Specific value: `"RAW"`

##

#### Path

Type: string Default: "127.0.0.1"

Path must not contain "{", "}" characters.

Must match regular expression: `^[^{}]*$`

Must be at least `1` characters long

##

#### Type

Type: enum (of string) Default: "AHCI"

Disk controller interface type. AHCI for compatibility, VIRTIO for performance.

##### Must be one of:

- "AHCI"
- "VIRTIO"

##

#### Exists

Type: boolean Default: false

Whether the disk file already exists or should be created.

##

#### Boot

Type: boolean Default: false

Whether this disk should be marked as bootable.

##

#### Size

Default: null

Size of the disk in bytes. Required if creating a new disk file.

## Any of

Type: integer
Type: null

##

#### Logical Sectorsize

Default: null

Logical sector size for the disk. `null` for default.

## Any of

Type: enum (of integer or null)

##### Must be one of:

- null
- 512
- 4096

Type: null

##

#### Physical Sectorsize

Default: null

Physical sector size for the disk. `null` for default.

## Any of

Type: enum (of integer or null)

##### Must be one of:

- null
- 512
- 4096

Type: null

##

#### Iotype

Type: enum (of string) Default: "THREADS"

I/O backend type for disk operations.

##### Must be one of:

- "NATIVE"
- "THREADS"
- "IO_URING"

##

#### Serial

Default: null

Serial number to assign to the virtual disk. `null` for auto-generated.

## Any of

Type: string

Must be at least `1` characters long

Type: null

#### VMDiskDevice

Type: object
No Additional Properties

##

#### Dtype

Type: const

Device type identifier for virtual disk devices.

Specific value: `"DISK"`

##

#### Path

Default: null

Path to existing disk file or ZFS volume. `null` if creating a new ZFS volume.

## Any of

Type: string

Must be at least `1` characters long

Type: null

##

#### Type

Type: enum (of string) Default: "AHCI"

Disk controller interface type. AHCI for compatibility, VIRTIO for performance.

##### Must be one of:

- "AHCI"
- "VIRTIO"

##

#### Create Zvol

Type: boolean Default: false

Whether to create a new ZFS volume for this disk.

##

#### Zvol Name

Default: null

Name for the new ZFS volume. Required if `create_zvol` is true.

## Any of

Type: string
Type: null

##

#### Zvol Volsize

Default: null

Size of the new ZFS volume in bytes. Required if `create_zvol` is true.

## Any of

Type: integer
Type: null

##

#### Logical Sectorsize

Default: null

Logical sector size for the disk. `null` for default.

## Any of

Type: enum (of integer or null)

##### Must be one of:

- null
- 512
- 4096

Type: null

##

#### Physical Sectorsize

Default: null

Physical sector size for the disk. `null` for default.

## Any of

Type: enum (of integer or null)

##### Must be one of:

- null
- 512
- 4096

Type: null

##

#### Iotype

Type: enum (of string) Default: "THREADS"

I/O backend type for disk operations.

##### Must be one of:

- "NATIVE"
- "THREADS"
- "IO_URING"

##

#### Serial

Default: null

Serial number to assign to the virtual disk. `null` for auto-generated.

## Any of

Type: string

Must be at least `1` characters long

Type: null

#### VMUSBDevice

Type: object
No Additional Properties

##

#### Dtype

Type: const

Device type identifier for USB devices.

Specific value: `"USB"`

##

Default: null

USB device attributes for identification. `null` for USB host controller only.

## Any of

#### USBAttributes

Type: object
No Additional Properties

##

#### Vendor Id

Type: string Default: "127.0.0.1"

USB vendor identifier in hexadecimal format (e.g., '0x1d6b' for Linux Foundation).

Must match regular expression: `^0x.*`

Must be at least `1` characters long

##

#### Product Id

Type: string Default: "127.0.0.1"

USB product identifier in hexadecimal format (e.g., '0x0002' for 2.0 root hub).

Must match regular expression: `^0x.*`

Must be at least `1` characters long

Type: null

##

#### Controller Type

Type: enum (of string) Default: "nec-xhci"

USB controller type for the virtual machine.

##### Must be one of:

- "piix3-uhci"
- "piix4-uhci"
- "ehci"
- "ich9-ehci1"
- "vt82c686b-uhci"
- "pci-ohci"
- "nec-xhci"
- "qemu-xhci"

##

#### Device

Default: null

Host USB device path to pass through. `null` for controller only.

## Any of

Type: string

Must be at least `1` characters long

Type: null

##

#### Vm

Type: integer

ID of the virtual machine this device belongs to.

##

#### Order

Type: integer

Boot order priority for this device (lower numbers boot first).

Required roles: VM_DEVICE_READ