# iscsi.target.update

Update iSCSI Target of id.

Type: object

##

Type: array
No Additional Items

#### Tuple Validation

##### Parameter 1: id

#### id

Type: integer

##### Parameter 2: iscsi_target_update

#### iscsi_target_update

Type: object
No Additional Properties

##

#### Name

Type: string

Must be at least `1` characters long

Must be at most `120` characters long

##

#### Alias

## Any of

Type: string
Type: null

##

#### Mode

Type: enum (of string)

##### Must be one of:

- "ISCSI"
- "FC"
- "BOTH"

##

#### Groups

Type: array of object
No Additional Items

##### Each item of this array must be:

#### IscsiGroup

Type: object
No Additional Properties

##

#### Portal

Type: integer

##

#### Initiator

Default: null

## Any of

Type: integer
Type: null

##

#### Authmethod

Type: enum (of string) Default: "NONE"

##### Must be one of:

- "NONE"
- "CHAP"
- "CHAP_MUTUAL"

##

#### Auth

Default: null

## Any of

Type: integer
Type: null

##

#### Auth Networks

Type: array of string
No Additional Items

##### Each item of this array must be:

Type: string

##

## Any of

#### IscsiTargetParameters

Type: object
No Additional Properties

##

#### Queuedcommands

Default: null

## Any of

Type: enum (of integer)

##### Must be one of:

- 32
- 128

Type: null
Type: null

##

#### iSCSITargetEntry

Type: object
No Additional Properties

##

#### Id

Type: integer

##

#### Name

Type: string

Must be at least `1` characters long

Must be at most `120` characters long

##

#### Alias

Default: null

## Any of

Type: string
Type: null

##

#### Mode

Type: enum (of string) Default: "ISCSI"

##### Must be one of:

- "ISCSI"
- "FC"
- "BOTH"

##

#### Groups

Type: array of object Default: []
No Additional Items

##### Each item of this array must be:

#### IscsiGroup

Type: object
No Additional Properties

##

#### Portal

Type: integer

##

#### Initiator

Default: null

## Any of

Type: integer
Type: null

##

#### Authmethod

Type: enum (of string) Default: "NONE"

##### Must be one of:

- "NONE"
- "CHAP"
- "CHAP_MUTUAL"

##

#### Auth

Default: null

## Any of

Type: integer
Type: null

##

#### Auth Networks

Type: array of string Default: []
No Additional Items

##### Each item of this array must be:

Type: string

##

#### Rel Tgt Id

Type: integer

##

Default: null

## Any of

#### IscsiTargetParameters

Type: object
No Additional Properties

##

#### Queuedcommands

Default: null

## Any of

Type: enum (of integer)

##### Must be one of:

- 32
- 128

Type: null
Type: null

Required roles: SHARING_ISCSI_TARGET_WRITE