# fcport.port_choices

Type: object

##

Type: array
No Additional Items

#### Tuple Validation

##### Parameter 1: include_used

#### include_used

Type: boolean Default: true

Whether to include FC ports that are already in use.

##

#### Result

Type: object
Example:

    {
        "fc0": {
            "wwpn": "naa.2100001122334455",
            "wwpn_b": "naa.210000AABBCCDDEEFF"
        },
        "fc0/1": {
            "wwpn": "naa.2200001122334455",
            "wwpn_b": "naa.220000AABBCCDDEEFF"
        }
    }

##

## Pattern Property

All properties whose name matches the following regular expression must respect the following conditions

Property name regular expression: `^[a-zA-Z0-9,\-_:]+(/[1-9][0-9]*)?$`

#### FCPortChoiceEntry

Type: object
No Additional Properties

##

#### Wwpn

World Wide Port Name for port A or `null` if not available.

## Any of

Type: string
Must match regular expression: `^naa.[0-9a-fA-F]{16}$`
Type: null

##

#### Wwpn B

World Wide Port Name for port B or `null` if not available.

## Any of

Type: string
Must match regular expression: `^naa.[0-9a-fA-F]{16}$`
Type: null

Required roles: READONLY_ADMIN | SHARING_ISCSI_TARGET_READ