# interface.lag_ports_choices

Return available interface choices that can be added to a bond (lag) interface.

Type: object

##

Type: array
No Additional Items

#### Tuple Validation

##### Parameter 1: id

#### id

Default: null

Name of existing bond interface whose member interfaces should be included in the result.

## Any of

Type: string
Type: null

##

#### Result

Type: object

IDs of available interfaces that can be added to a bond interface.

##

Each additional property must conform to the following schema

Type: string

Required roles: NETWORK_INTERFACE_READ | READONLY_ADMIN