# jbof.reapply_config

Reapply the JBOF configuration to attached JBOFs.

If an IOM is replaced in a JBOF, then it is expected to be configured to have the same redfish IP, user & password as was previously the case.

This API can then be called to configure each JBOF with the expected data-plane IP configuration, and then attach NVMe drives.

Type: object

##

Type: array
No Additional Items

##

#### Result

Type: null

Returns `null` when the JBOF configuration is successfully reapplied.

Required roles: JBOF_WRITE