# jbof.update

Update JBOF of id

Type: object

##

Type: array
No Additional Items

#### Tuple Validation

##### Parameter 1: id

#### id

Type: integer

ID of the JBOF to update.

##### Parameter 2: data

#### data

Type: object

Updated JBOF configuration data.

No Additional Properties

##

#### Description

Type: string

Optional description of the JBOF.

##

#### Mgmt Ip1

IP of first Redfish management interface.

## Any of

Type: const
Specific value: `""`
Type: string

##

#### Mgmt Ip2

Optional IP of second Redfish management interface.

## Any of

Type: const
Specific value: `""`
Type: string

##

#### Mgmt Username

Type: string

Redfish administrative username.

##

#### Mgmt Password

Type: string

Redfish administrative password.

##

#### JBOFEntry

Type: object

The updated JBOF configuration.

No Additional Properties

##

#### Id

Type: integer

Unique identifier for the JBOF configuration.

##

#### Description

Type: string

Optional description of the JBOF.

##

#### Mgmt Ip1

IP of first Redfish management interface.

## Any of

Type: const
Specific value: `""`
Type: string

##

#### Mgmt Ip2

Optional IP of second Redfish management interface.

## Any of

Type: const
Specific value: `""`
Type: string

##

#### Mgmt Username

Type: string

Redfish administrative username.

##

#### Mgmt Password

Type: string

Redfish administrative password.

##

#### Index

Type: integer

Index of the JBOF. Used to determine data plane IP addresses.

##

#### Uuid

Type: string

UUID of the JBOF as reported by the enclosure firmware.

Required roles: JBOF_WRITE