# nfs.config

Type: object

##

Type: array
No Additional Items

##

#### NFSEntry

Type: object
No Additional Properties

##

#### Id

Type: integer

Placeholder identifier. Not used as there is only one.

##

#### Servers

Specify the number of nfsd. Default: Number of nfsd is equal number of CPU.

## Any of

Type: integer

Value must be greater or equal to `1` and lesser or equal to `256`

Type: null

##

#### Allow Nonroot

Type: boolean

Allow non-root mount requests. This equates to 'insecure' share option.

##

#### Protocols

Type: array of enum (of string)

Specify supported NFS protocols: NFSv3, NFSv4 or both can be listed.

No Additional Items

##### Each item of this array must be:

Type: enum (of string)

##### Must be one of:

- "NFSV3"
- "NFSV4"

##

#### V4 Krb

Type: boolean

Force Kerberos authentication on NFS shares.

##

#### V4 Domain

Type: string

Specify a DNS domain (NFSv4 only).

##

#### Bindip

Type: array of string Default: []

Limit the server IP addresses available for NFS.

No Additional Items

##### Each item of this array must be:

Type: string

Must be at least `1` characters long

##

#### Mountd Port

Specify the mountd port binding.

## Any of

Type: integer

Value must be greater or equal to `1` and lesser or equal to `65535`

Type: null

##

#### Rpcstatd Port

Specify the rpc.statd port binding.

## Any of

Type: integer

Value must be greater or equal to `1` and lesser or equal to `65535`

Type: null

##

#### Rpclockd Port

Specify the rpc.lockd port binding.

## Any of

Type: integer

Value must be greater or equal to `1` and lesser or equal to `65535`

Type: null

##

#### Mountd Log

Type: boolean

Enable or disable mountd logging.

##

#### Statd Lockd Log

Type: boolean

Enable or disable statd and lockd logging.

##

#### V4 Krb Enabled

Type: boolean

Status of NFSv4 authentication requirement (status only).

##

#### Userd Manage Gids

Type: boolean

Enable to allow server to manage gids.

##

#### Keytab Has Nfs Spn

Type: boolean

Report status of NFS Principal Name in keytab (status only).

##

#### Managed Nfsd

Type: boolean

Report status of 'servers' field. If true, the number of nfsd is managed by the server (status only).

##

#### Rdma

Type: boolean

Enable or disable NFS over RDMA. Requires RDMA capable NIC.

Required roles: SHARING_NFS_READ